(module Battery_Keystone_590_596_1xAA (layer F.Cu) (tedit 5E8F4FA2)
  (fp_text reference REF** (at 0 2) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Battery_Keystone_590_596_1xAA (at 0 -1.5) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -23 0) (end -19 0) (layer F.SilkS) (width 0.3))
  (fp_line (start 23 0) (end 19 0) (layer F.SilkS) (width 0.3))
  (fp_line (start 21 -2) (end 21 2) (layer F.SilkS) (width 0.3))
  (fp_line (start -15 -4) (end -15 4) (layer F.SilkS) (width 0.3))
  (fp_line (start -15 4) (end 15 4) (layer F.SilkS) (width 0.3))
  (fp_line (start 15 4) (end 15 2) (layer F.SilkS) (width 0.3))
  (fp_line (start 15 2) (end 16 2) (layer F.SilkS) (width 0.3))
  (fp_line (start 16 2) (end 16 -2) (layer F.SilkS) (width 0.3))
  (fp_line (start 16 -2) (end 15 -2) (layer F.SilkS) (width 0.3))
  (fp_line (start 15 -2) (end 15 -4) (layer F.SilkS) (width 0.3))
  (fp_line (start 15 -4) (end -15 -4) (layer F.SilkS) (width 0.3))
  (fp_line (start -33 -7.5) (end -33 7.5) (layer F.CrtYd) (width 0.12))
  (fp_line (start -33 7.5) (end 33 7.5) (layer F.CrtYd) (width 0.12))
  (fp_line (start 33 7.5) (end 33 -7.5) (layer F.CrtYd) (width 0.12))
  (fp_line (start 33 -7.5) (end -33 -7.5) (layer F.CrtYd) (width 0.12))
  (pad 1 thru_hole rect (at 26.29 0) (size 2.4 2.4) (drill 1.4) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at 29.34 -4.45) (size 2.4 2.4) (drill 1.4) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at 29.34 4.45) (size 2.4 2.4) (drill 1.4) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at -26.29 0) (size 2.4 2.4) (drill 1.4) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at -29.34 -4.45) (size 2.4 2.4) (drill 1.4) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at -29.34 4.45) (size 2.4 2.4) (drill 1.4) (layers *.Cu *.Mask))
)
