(module Pin_Header_Side_1x14_Pitch2.54mm_SMD (layer F.Cu) (tedit 5E7A229D)
  (fp_text reference REF** (at 0 -2.54) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Pin_Header_Side_1x14_Pitch2.54mm_SMD (at 0 2.54) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user 1 (at -16.51 -2.54) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad 1 smd rect (at -16.51 0) (size 1.5 3) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -13.97 0) (size 1.5 3) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -11.43 0) (size 1.5 3) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -8.89 0) (size 1.5 3) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at -6.35 0) (size 1.5 3) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at -3.81 0) (size 1.5 3) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at -1.27 0) (size 1.5 3) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at 1.27 0) (size 1.5 3) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at 3.81 0) (size 1.5 3) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at 6.35 0) (size 1.5 3) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd rect (at 8.89 0) (size 1.5 3) (layers F.Cu F.Paste F.Mask))
  (pad 12 smd rect (at 11.43 0) (size 1.5 3) (layers F.Cu F.Paste F.Mask))
  (pad 13 smd rect (at 13.97 0) (size 1.5 3) (layers F.Cu F.Paste F.Mask))
  (pad 14 smd rect (at 16.51 0) (size 1.5 3) (layers F.Cu F.Paste F.Mask))
)
