EESchema-DOCLIB  Version 2.0
#
$CMP GY-B11_EP_280
D Breakout board for BME280, 3-in-1 sensor, humidity, pressure, temperature, I2C and SPI interface, 1.71-3.6V, LGA-8
K Bosch pressure humidity temperature environment environmental measurement digital
F https://ae-bst.resource.bosch.com/media/_tech/media/datasheets/BST-BME280-DS002.pdf
$ENDCMP
#
#End Doc Library
