EESchema-DOCLIB  Version 2.0
#
$CMP BU49xx
K supply voltage supervisor
F https://fscdn.rohm.com/en/products/databook/datasheet/ic/power/voltage_detector/bd48xxg-e.pdf
$ENDCMP
#
$CMP GY-B11_EP_280
D Breakout board for BME280, 3-in-1 sensor, humidity, pressure, temperature, I2C and SPI interface, 1.71-3.6V, LGA-8
K Bosch pressure humidity temperature environment environmental measurement digital
F https://ae-bst.resource.bosch.com/media/_tech/media/datasheets/BST-BME280-DS002.pdf
$ENDCMP
#
$CMP NRF24L01_Breakout_SMD
D Ultra low power 2.4GHz RF Transceiver, Carrier PCB, SMD
K Low Power RF Transciever breakout carrier SMD
F http://www.nordicsemi.com/eng/content/download/2730/34105/file/nRF24L01_Product_Specification_v2_0.pdf
$ENDCMP
#
#End Doc Library
