(module aaa_holder_keystone_591+597 (layer F.Cu) (tedit 5E7A314B)
  (descr "Footprint for a AAA-battery holder using the Keystone 591 and 597")
  (fp_text reference REF** (at 0 11.43) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value aaa_holder_keystone_591+597 (at 0 8.89) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -17 0) (end -20 0) (layer F.SilkS) (width 0.3))
  (fp_line (start 18.5 -1.5) (end 18.5 1.5) (layer F.SilkS) (width 0.3))
  (fp_line (start 20 0) (end 17 0) (layer F.SilkS) (width 0.3))
  (fp_line (start 15 1.5) (end 15 -1.5) (layer F.SilkS) (width 0.3))
  (fp_line (start 14 1.5) (end 15 1.5) (layer F.SilkS) (width 0.3))
  (fp_line (start 14 3.5) (end 14 1.5) (layer F.SilkS) (width 0.3))
  (fp_line (start -15 3.5) (end 14 3.5) (layer F.SilkS) (width 0.3))
  (fp_line (start -15 -3.5) (end -15 3.5) (layer F.SilkS) (width 0.3))
  (fp_line (start 14 -3.5) (end -15 -3.5) (layer F.SilkS) (width 0.3))
  (fp_line (start 14 -1.5) (end 14 -3.5) (layer F.SilkS) (width 0.3))
  (fp_line (start 15 -1.5) (end 14 -1.5) (layer F.SilkS) (width 0.3))
  (fp_line (start -29.75 -5.5) (end -29.75 5.5) (layer F.CrtYd) (width 0.12))
  (fp_line (start -29.75 5.5) (end 29.75 5.5) (layer F.CrtYd) (width 0.12))
  (fp_line (start 29.75 5.5) (end 29.75 -5.5) (layer F.CrtYd) (width 0.12))
  (fp_line (start 29.75 -5.5) (end -29.75 -5.5) (layer F.CrtYd) (width 0.12))
  (pad 1 thru_hole circle (at 26.25 4.45) (size 3 3) (drill 1.3) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at 26.25 -4.45) (size 3 3) (drill 1.3) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at -26.25 4.45) (size 3 3) (drill 1.3) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at -26.25 -4.45) (size 3 3) (drill 1.3) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at -23.25 0) (size 3 3) (drill 1.3) (layers *.Cu *.Mask))
  (pad 1 thru_hole rect (at 23.25 0) (size 3 3) (drill 1.3) (layers *.Cu *.Mask))
)
