(module NRF24L01+breakout_SMD (layer F.Cu) (tedit 5E78B67B)
  (fp_text reference REF** (at 0 0.5) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value NRF24L01+breakout_SMD (at 0 -0.5) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 6 -1.5) (end -6 -1.5) (layer F.SilkS) (width 0.15))
  (fp_line (start -6 9) (end -6 -9) (layer F.SilkS) (width 0.15))
  (fp_line (start 6 9) (end -6 9) (layer F.SilkS) (width 0.15))
  (fp_line (start 6 -9) (end 6 9) (layer F.SilkS) (width 0.15))
  (fp_line (start -6 -9) (end 6 -9) (layer F.SilkS) (width 0.15))
  (pad 1 smd rect (at -4.445 9) (size 1 3) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -3.175 9) (size 1 3) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -1.905 9) (size 1 3) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -0.635 9) (size 1 3) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 0.635 9) (size 1 3) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 1.905 9) (size 1 3) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at 3.175 9) (size 1 3) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at 4.445 9) (size 1 3) (layers F.Cu F.Paste F.Mask))
  (pad "" thru_hole rect (at 5.1 -2.5) (size 1.8 1) (drill 0.6) (layers *.Cu *.Mask))
)
