(module GY-B11_EP_280_SMD (layer F.Cu) (tedit 5E7A31C0)
  (attr smd)
  (fp_text reference REF** (at 0 -7) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value GY-B11_EP_280_SMD (at 0 7) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -8 -6) (end -8 6) (layer F.SilkS) (width 0.15))
  (fp_line (start -8 6) (end 8 6) (layer F.SilkS) (width 0.15))
  (fp_line (start 8 6) (end 8 -6) (layer F.SilkS) (width 0.15))
  (fp_line (start 8 -6) (end -8 -6) (layer F.SilkS) (width 0.15))
  (fp_line (start -8.2 -6.2) (end -8.2 6.2) (layer F.CrtYd) (width 0.12))
  (fp_line (start -8.2 6.2) (end 8.2 6.2) (layer F.CrtYd) (width 0.12))
  (fp_line (start 8.2 6.2) (end 8.2 -6.2) (layer F.CrtYd) (width 0.12))
  (fp_line (start 8.2 -6.2) (end -8.2 -6.2) (layer F.CrtYd) (width 0.12))
  (pad 2 smd circle (at -3.73 5) (size 2 2) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd circle (at -1.27 5) (size 2 2) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd circle (at 1.27 5) (size 2 2) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd circle (at 3.81 5) (size 2 2) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd circle (at 6.35 5) (size 2 2) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at -6.35 5) (size 2 2) (layers F.Cu F.Paste F.Mask))
  (pad "" smd circle (at 5.08 -2.62) (size 5 5) (layers F.Cu F.Paste F.Mask))
  (pad "" smd circle (at -5.08 -2.62) (size 5 5) (layers F.Cu F.Paste F.Mask))
)
