(module "Fuseholder_Littlefuse_NANO2-154" (layer "F.Cu") (tedit 5FB1896C)
  (descr "Littlefuse NANO2 154 OMNI-BLOK fuse holder")
  (tags "fuse holder littlefuse nano2 154 omni blok")
  (attr smd)
  (fp_text reference "REF**" (at 0 -3.2 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 2d273b78-bc0d-4b61-8fa2-8adf93fda753)
  )
  (fp_text value "Fuseholder_Littlefuse_NANO2-154" (at 0 3.3 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 4dd9f4cc-ae11-4877-ad3e-e69bfa07c03d)
  )
  (fp_text user "${REFERENCE}" (at 0 0 90 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 818e3c90-2985-4447-ab79-33561411aaa2)
  )
  (fp_line (start 5.3 2.5) (end 5.3 2.1) (layer "F.SilkS") (width 0.12) (tstamp 0e7a95f5-7ff8-4a31-84d4-66cc607dd07b))
  (fp_line (start -5.3 2.1) (end -5.3 2.5) (layer "F.SilkS") (width 0.12) (tstamp 2668ea59-ae5a-434d-ae8e-87846c8b6e56))
  (fp_line (start -5.3 -2.5) (end 5.3 -2.5) (layer "F.SilkS") (width 0.12) (tstamp 6cd7a572-60ee-47ff-941e-8a37a81bc334))
  (fp_line (start -5.3 2.5) (end 5.3 2.5) (layer "F.SilkS") (width 0.12) (tstamp b59206e9-da60-4291-895c-e09fa76cb631))
  (fp_line (start -5.3 -2.5) (end -5.3 -2.1) (layer "F.SilkS") (width 0.12) (tstamp c271efde-0569-4ebe-94ae-986bb38b2e04))
  (fp_line (start 5.3 -2.5) (end 5.3 -2.1) (layer "F.SilkS") (width 0.12) (tstamp cafea76c-638d-4bab-931f-177a1fe47036))
  (fp_line (start 5.3 -2.5) (end 5.3 2.5) (layer "F.Fab") (width 0.1) (tstamp a40c1fd1-29fa-49b7-b100-378ebaad45ee))
  (fp_line (start 5.3 2.5) (end -5.3 2.5) (layer "F.Fab") (width 0.1) (tstamp b1d93d4f-e430-429f-916d-bdd8ddc622ac))
  (fp_line (start -5.3 2.5) (end -5.3 -2.5) (layer "F.Fab") (width 0.1) (tstamp e8560fa9-39bc-4eb5-a386-40c902f89c98))
  (fp_line (start -5.3 -2.5) (end 5.3 -2.5) (layer "F.Fab") (width 0.1) (tstamp eff1dbe6-714b-46d5-8a43-ccd247869b7d))
  (pad "1" smd rect (at -3.19 0) (size 4.24 3.81) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp e990530a-5534-4bec-a66b-7f5a0ecece3f))
  (pad "2" smd rect (at 3.19 0) (size 4.24 3.81) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp b20abd7d-a06e-4945-9533-963c8fb59f6e))
)
