(footprint "TE_796638-2_1x02_P5.08mm_Horizontal" (version 20201116) (generator pcbnew) (layer "F.Cu")
  (tedit 5FC96F58)
  (descr "TE Connectivity 796638-2 Pluggable Terminal Block")
  (tags "TE connectivity 796638-2 pluggable terminal block 5.08mm")
  (attr through_hole)
  (fp_text reference "REF**" (at 2.54 -2.7 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp b4e9cc8a-0aaa-4077-8a4c-b86d841c63f7)
  )
  (fp_text value "TE_796638-2_1x02_P5.08mm_Horizontal" (at 2.54 10.86 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 6936aee9-d49a-4519-86d6-d19aa1d28e99)
  )
  (fp_text user "${REFERENCE}" (at 2.54 2.49 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 16461a3e-6e7d-4868-acc8-4931271a443a)
  )
  (fp_line (start -3.7 -2) (end 8.28 -2) (layer "F.SilkS") (width 0.12) (tstamp 1384be3d-3d5f-4142-b75c-b7d6a70ff3dc))
  (fp_line (start 8.28 -2) (end 8.28 10) (layer "F.SilkS") (width 0.12) (tstamp 4d50868f-9685-48c9-9834-fb45e1bb63c2))
  (fp_line (start 8.28 10) (end -3.7 10) (layer "F.SilkS") (width 0.12) (tstamp 683bd1e8-d6e7-418d-81f6-27995d02d529))
  (fp_line (start -3.7 10) (end -3.7 -2) (layer "F.SilkS") (width 0.12) (tstamp a554a02b-537b-4f18-8840-91121883c4a9))
  (fp_rect (start -4.2 -2.5) (end 8.78 10.5) (layer "F.CrtYd") (width 0.12) (fill none) (tstamp c73c097a-c545-44c2-97d9-4b7e65a893bb))
  (fp_rect (start -3.7 -2) (end 8.28 10) (layer "F.Fab") (width 0.1) (fill none) (tstamp c7864f87-2828-475b-80cb-44ff58b71ee6))
  (pad "1" thru_hole circle (at 0 0) (size 3 3) (drill 1.4) (layers *.Cu *.Mask) (tstamp 2e345f08-bcb6-4d06-b0f4-f62e75da38c0))
  (pad "2" thru_hole circle (at 5.08 0) (size 3 3) (drill 1.4) (layers *.Cu *.Mask) (tstamp 03e7c998-a23c-45f8-8cf4-78ffcf7e014f))
  (model "/home/mathias/Projects/microcontroller/HackAmp/3dmodels/c-796638-2-c3-3d.stp"
    (offset (xyz 2.3 -10 3.85))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
