(kicad_symbol_lib (version 20201005) (generator kicad_symbol_editor)
  (symbol "HackAmp-Symbols:AudioJack4_Ground_IsolatedSwitch" (in_bom yes) (on_board yes)
    (property "Reference" "J" (id 0) (at 0 11.43 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "AudioJack4_Ground_IsolatedSwitch" (id 1) (at 0 8.89 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (id 2) (at -1.27 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (id 3) (at -1.27 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "audio jack receptacle stereo headphones phones TRS connector" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Audio Jack, 4 Poles (Stereo / TRRS), Grounded Sleeve, Switched TR1 Poles (Normalling)" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "Jack*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "AudioJack4_Ground_IsolatedSwitch_0_1"
      (rectangle (start -7.62 -2.54) (end -8.89 -5.08)
        (stroke (width 0.254)) (fill (type outline))
      )
      (rectangle (start -7.62 6.35) (end 3.81 -10.16)
        (stroke (width 0.254)) (fill (type background))
      )
      (polyline
        (pts
          (xy 3.81 2.54)
          (xy 5.08 2.54)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy 5.08 -2.54)
          (xy 3.81 -2.54)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy 5.08 0)
          (xy 3.81 0)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy 5.08 5.08)
          (xy 3.81 5.08)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy 5.08 -5.08)
          (xy 1.905 -5.08)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy 1.905 -5.08)
          (xy 1.905 -4.826)
        )
        (stroke (width 0.001)) (fill (type none))
      )
      (polyline
        (pts
          (xy 1.905 -2.921)
          (xy 1.905 -2.54)
        )
        (stroke (width 0.001)) (fill (type none))
      )
      (polyline
        (pts
          (xy 1.905 -4.445)
          (xy 1.905 -4.064)
        )
        (stroke (width 0.001)) (fill (type none))
      )
      (polyline
        (pts
          (xy 1.905 -3.683)
          (xy 1.905 -3.302)
        )
        (stroke (width 0.001)) (fill (type none))
      )
      (polyline
        (pts
          (xy 2.286 -2.921)
          (xy 2.286 -2.54)
        )
        (stroke (width 0.001)) (fill (type none))
      )
      (polyline
        (pts
          (xy 2.286 -5.08)
          (xy 2.286 -4.826)
        )
        (stroke (width 0.001)) (fill (type none))
      )
      (polyline
        (pts
          (xy 2.286 -4.445)
          (xy 2.286 -4.064)
        )
        (stroke (width 0.001)) (fill (type none))
      )
      (polyline
        (pts
          (xy 2.286 -3.683)
          (xy 2.286 -3.302)
        )
        (stroke (width 0.001)) (fill (type none))
      )
    )
    (symbol "AudioJack4_Ground_IsolatedSwitch_1_1"
      (polyline
        (pts
          (xy 3.048 -5.334)
          (xy 3.302 -5.842)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy -1.27 -2.54)
          (xy -0.635 -3.175)
          (xy 0 -2.54)
          (xy 3.81 -2.54)
        )
        (stroke (width 0.254)) (fill (type none))
      )
      (polyline
        (pts
          (xy 5.08 -7.62)
          (xy 3.048 -7.62)
          (xy 3.048 -5.334)
          (xy 2.794 -5.842)
        )
        (stroke (width 0)) (fill (type none))
      )
      (polyline
        (pts
          (xy -3.175 -2.54)
          (xy -2.54 -3.175)
          (xy -1.905 -2.54)
          (xy -1.905 0)
          (xy 3.81 0)
        )
        (stroke (width 0.254)) (fill (type none))
      )
      (polyline
        (pts
          (xy 3.81 2.54)
          (xy -3.81 2.54)
          (xy -3.81 -2.54)
          (xy -4.445 -3.175)
          (xy -5.08 -2.54)
        )
        (stroke (width 0.254)) (fill (type none))
      )
      (polyline
        (pts
          (xy 3.81 5.08)
          (xy -5.715 5.08)
          (xy -5.715 -2.54)
          (xy -6.35 -3.175)
          (xy -6.985 -2.54)
        )
        (stroke (width 0.254)) (fill (type none))
      )
      (pin passive line (at 0 -12.7 90) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "G" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 7.62 0 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "R1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 7.62 2.54 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "R2" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 7.62 5.08 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "S" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 7.62 -2.54 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "T" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 7.62 -7.62 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "SW1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 7.62 -5.08 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "SW2" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "HackAmp-Symbols:CSR-A64215-MOD" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -15.24 39.37 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "CSR-A64215-MOD" (id 1) (at 8.89 39.37 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (id 2) (at 6.35 -7.62 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (id 3) (at 6.35 -7.62 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "CSR-A64215-MOD_0_1"
      (rectangle (start -17.78 38.1) (end 17.78 -35.56)
        (stroke (width 0)) (fill (type background))
      )
    )
    (symbol "CSR-A64215-MOD_1_1"
      (pin bidirectional line (at -20.32 2.54 0) (length 2.54)
        (name "PIO6" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 0 0) (length 2.54)
        (name "PIO7" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -2.54 0) (length 2.54)
        (name "PIO8/UART_RTS" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -5.08 0) (length 2.54)
        (name "PIO9/UART_CTS" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -12.7 0) (length 2.54)
        (name "PIO18" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -15.24 0) (length 2.54)
        (name "PIO21" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -20.32 -33.02 0) (length 2.54)
        (name "SPI/~PCM" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 12.7 0) (length 2.54)
        (name "PIO2/PCM1_IN/SPI_MOSI" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 5.08 0) (length 2.54)
        (name "PIO5/PCM1_CLK/SPI_CLK" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 7.62 0) (length 2.54)
        (name "PIO4/PCM1_SYNC/SPI_CS" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 10.16 0) (length 2.54)
        (name "PIO3/PCM1_OUT/SPI_MISO" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 20.32 30.48 180) (length 2.54)
        (name "~RST" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -20.32 27.94 0) (length 2.54)
        (name "VBAT" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -38.1 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 5.08 180) (length 2.54)
        (name "USBN" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 22.86 0) (length 2.54)
        (name "VREGENABLE/MFB" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 20.32 15.24 180) (length 2.54)
        (name "1V8" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -20.32 -17.78 0) (length 2.54)
        (name "PIO29/LED0" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -20.32 -20.32 0) (length 2.54)
        (name "PIO30/LED1" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -20.32 -22.86 0) (length 2.54)
        (name "PIO31/LED2" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -20.32 180) (length 2.54)
        (name "MICAN" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -17.78 180) (length 2.54)
        (name "MICAP" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -15.24 180) (length 2.54)
        (name "MIC_BIAS" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -27.94 180) (length 2.54)
        (name "LIBN" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -25.4 180) (length 2.54)
        (name "LIBP" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -2.54 180) (length 2.54)
        (name "RN" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 0 180) (length 2.54)
        (name "RP" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -10.16 180) (length 2.54)
        (name "LN" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -7.62 180) (length 2.54)
        (name "LP" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -10.16 0) (length 2.54)
        (name "PIO17/UART_CTS" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -7.62 0) (length 2.54)
        (name "PIO16/UART_RTS" (effects (font (size 1.27 1.27))))
        (number "38" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 20.32 12.7 180) (length 2.54)
        (name "USB3V3" (effects (font (size 1.27 1.27))))
        (number "39" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 22.86 180) (length 2.54)
        (name "ANT" (effects (font (size 1.27 1.27))))
        (number "40" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 20.32 180) (length 2.54)
        (name "ANT_GND" (effects (font (size 1.27 1.27))))
        (number "41" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -20.32 35.56 0) (length 2.54)
        (name "VCHG" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -20.32 30.48 0) (length 2.54)
        (name "EXT" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -20.32 33.02 0) (length 2.54)
        (name "SENSE" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 7.62 180) (length 2.54)
        (name "USBP" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -20.32 -27.94 0) (length 2.54)
        (name "AIO0" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 15.24 0) (length 2.54)
        (name "PIO1/UART_TX" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 17.78 0) (length 2.54)
        (name "PIO0/UART_RX" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "HackAmp-Symbols:TAS5760M" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -7.62 31.75 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Value" "TAS5760M" (id 1) (at 5.08 31.75 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Footprint" "" (id 2) (at 0 12.7 0)
      (effects (font (size 1.524 1.524)) hide)
    )
    (property "Datasheet" "https://www.ti.com/lit/ds/symlink/tas5760m.pdf" (id 3) (at 0 12.7 0)
      (effects (font (size 1.524 1.524)) hide)
    )
    (property "ki_keywords" "tas5760m i2s class-d audio amplifier" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "TAS5760M General-Purpose I2S Input Class-D Amplifier" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "TAS5760M_1_1"
      (rectangle (start -15.24 -30.48) (end 15.24 30.48)
        (stroke (width 0)) (fill (type background))
      )
      (pin power_in line (at 22.86 27.94 180) (length 7.62)
        (name "AVDD" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -22.86 27.94 0) (length 7.62)
        (name "DVDD" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -22.86 22.86 0) (length 7.62)
        (name "SPK_GAIN0" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -22.86 20.32 0) (length 7.62)
        (name "SPK_GAIN1" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -22.86 -7.62 0) (length 7.62)
        (name "SPK_SLEEP/ADR" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -22.86 -12.7 0) (length 7.62)
        (name "MCLK" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -22.86 -15.24 0) (length 7.62)
        (name "SCLK" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -22.86 -17.78 0) (length 7.62)
        (name "SDIN" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -22.86 -20.32 0) (length 7.62)
        (name "LRCK" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -22.86 -25.4 0) (length 7.62)
        (name "DGND" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 22.86 -2.54 180) (length 7.62)
        (name "BSTRPB+" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 22.86 -15.24 180) (length 7.62)
        (name "SFT_CLIP" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 22.86 -5.08 180) (length 7.62)
        (name "SPK_OUTB+" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 22.86 22.86 180) (length 7.62)
        (name "PVDD" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 22.86 -25.4 180) (length 7.62)
        (name "PGND" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 22.86 -7.62 180) (length 7.62)
        (name "SPK_OUTB-" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 22.86 -10.16 180) (length 7.62)
        (name "BSTRPB-" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 22.86 5.08 180) (length 7.62)
        (name "BSTRPA-" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 22.86 7.62 180) (length 7.62)
        (name "SPK_OUTA-" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 22.86 -27.94 180) (length 7.62)
        (name "PGND" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 22.86 20.32 180) (length 7.62)
        (name "PVDD" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 22.86 10.16 180) (length 7.62)
        (name "SPK_OUTA+" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -22.86 15.24 0) (length 7.62)
        (name "ANA_REG" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 22.86 12.7 180) (length 7.62)
        (name "BSTRPA+" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 22.86 -22.86 180) (length 7.62)
        (name "GGND" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 22.86 -17.78 180) (length 7.62)
        (name "GVDD_REG" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -22.86 -27.94 0) (length 7.62)
        (name "GND/PAD" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -22.86 12.7 0) (length 7.62)
        (name "VCOM" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -22.86 10.16 0) (length 7.62)
        (name "ANA_REF" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -22.86 5.08 0) (length 7.62)
        (name "~SPK_FAULT" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -22.86 2.54 0) (length 7.62)
        (name "~SPK_SD" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -22.86 -2.54 0) (length 7.62)
        (name "FREQ/SDA" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -22.86 -5.08 0) (length 7.62)
        (name "PBTL/SCL" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
)
