(footprint "PanelCutout_Jack_3.5mm_CUI_SJ-435107" (version 20201116) (generator pcbnew) (layer "F.Cu")
  (tedit 5FC20ACD)
  (fp_text reference "REF**" (at 0 -4.1 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp a24b419b-8527-4cdc-9137-b60ccafdfdd5)
  )
  (fp_text value "PanelCutout_Jack_3.5mm_CUI_SJ-435107" (at 0 -5.5 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 2b07aac2-43d6-417b-9b69-0a7ed6e634e5)
  )
  (fp_text user "${REFERENCE}" (at 0 -4.1 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 1baab8da-5d47-4da5-9866-ecb779be6ad3)
  )
  (fp_rect (start -5.6 -3.3) (end 5.2 4) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 68361ace-6af1-4443-9035-960d471ca04a))
  (fp_rect (start 5.7 -4.8) (end -6.1 6.9) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp b69bb4b7-297c-4421-8500-fa16265ca643))
  (fp_line (start 5.2 4) (end 5.2 6.4) (layer "F.Fab") (width 0.1) (tstamp 4c05a40c-04df-43f6-8da1-9d460ad0bb6a))
  (fp_line (start -5.6 4) (end -5.6 6.4) (layer "F.Fab") (width 0.1) (tstamp f66bd75e-7ac5-4fa7-b434-168276b8ad76))
  (fp_rect (start -5.6 -3.3) (end 5.2 4) (layer "F.Fab") (width 0.1) (fill none) (tstamp 1baffc9e-0afd-41e7-aa8d-6d69452d21ed))
  (fp_rect (start 3.9 -3.3) (end 2.4 -4.3) (layer "F.Fab") (width 0.1) (fill none) (tstamp 4304fa3b-1830-44c8-846f-8794826399bd))
  (fp_rect (start -4.3 -3.3) (end -2.8 -4.3) (layer "F.Fab") (width 0.1) (fill none) (tstamp 5e3acf0c-b80e-43ad-b20c-05e676ba6d62))
  (pad "" np_thru_hole circle (at 0 0) (size 6.2 6.2) (drill 6.2) (layers *.Mask) (tstamp e9d2b18d-0ca9-48f9-947b-819632e96dd0))
  (model "/home/mathias/Projects/microcontroller/HackAmp/3dmodels/CUI_DEVICES_SJ-435107RS.step"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 180 0))
  )
)
