(module Jack_3.5mm_Switchcraft_35RASMT4BHNTRX_Horizontal (layer F.Cu) (tedit 5FAF8FA9)
  (descr "Switchcraft 3.5mm TRS Phone Jack")
  (tags "switchcraft 3.5mm trs phone jack audio connector")
  (attr smd)
  (fp_text reference REF** (at 4 3 270) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Jack_3.5mm_Switchcraft_35RASMT4BHNTRX_Horizontal (at 6 0 90) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -3 7.5) (end 3 7.5) (layer F.Fab) (width 0.12))
  (fp_line (start -3 -7) (end -3 7.5) (layer F.Fab) (width 0.12))
  (fp_line (start -2.5 -7) (end -3 -7) (layer F.Fab) (width 0.12))
  (fp_line (start -2.5 -9.5) (end -2.5 -7) (layer F.Fab) (width 0.12))
  (fp_line (start 2.5 -9.5) (end -2.5 -9.5) (layer F.Fab) (width 0.12))
  (fp_line (start 2.5 -7) (end 2.5 -9.5) (layer F.Fab) (width 0.12))
  (fp_line (start 3 -7) (end 2.5 -7) (layer F.Fab) (width 0.12))
  (fp_line (start 3 7.5) (end 3 -7) (layer F.Fab) (width 0.12))
  (fp_line (start -3 7.5) (end -1.5 7.5) (layer F.SilkS) (width 0.15))
  (fp_line (start -3 7.5) (end -3 6.25) (layer F.SilkS) (width 0.15))
  (fp_line (start 1.5 7.5) (end 3 7.5) (layer F.SilkS) (width 0.15))
  (fp_line (start 3 7.5) (end 3 -1.5) (layer F.SilkS) (width 0.15))
  (fp_line (start -3 3.25) (end -3 -3.25) (layer F.SilkS) (width 0.15))
  (fp_line (start -3 -6) (end -3 -7) (layer F.SilkS) (width 0.15))
  (fp_line (start -3 -7) (end 3 -7) (layer F.SilkS) (width 0.15))
  (fp_line (start 3 -7) (end 3 -6.75) (layer F.SilkS) (width 0.15))
  (fp_text user %R (at 0 0 90) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 5.6 -1.1) (end 5.6 -7) (layer F.CrtYd) (width 0.12))
  (fp_line (start 5.6 -7) (end 3.5 -7) (layer F.CrtYd) (width 0.12))
  (fp_line (start 3.5 -7) (end 3.5 -7.5) (layer F.CrtYd) (width 0.12))
  (fp_line (start 3.5 -7.5) (end 3 -7.5) (layer F.CrtYd) (width 0.12))
  (fp_line (start 3 -7.5) (end 3 -10) (layer F.CrtYd) (width 0.12))
  (fp_line (start 3 -10) (end -3 -10) (layer F.CrtYd) (width 0.12))
  (fp_line (start -3 -10) (end -3 -7.5) (layer F.CrtYd) (width 0.12))
  (fp_line (start -3 -7.5) (end -3.5 -7.5) (layer F.CrtYd) (width 0.12))
  (fp_line (start -3.5 -7.5) (end -3.5 -6.2) (layer F.CrtYd) (width 0.12))
  (fp_line (start -3.5 -6.2) (end -5.6 -6.2) (layer F.CrtYd) (width 0.12))
  (fp_line (start -5.6 -6.2) (end -5.6 -3) (layer F.CrtYd) (width 0.12))
  (fp_line (start -5.6 -3) (end -3.5 -3) (layer F.CrtYd) (width 0.12))
  (fp_line (start -3.5 -3) (end -3.5 2.8) (layer F.CrtYd) (width 0.12))
  (fp_line (start -3.5 2.8) (end -5.6 2.8) (layer F.CrtYd) (width 0.12))
  (fp_line (start -5.6 2.8) (end -5.6 6.6) (layer F.CrtYd) (width 0.12))
  (fp_line (start -5.6 6.6) (end -3.5 6.6) (layer F.CrtYd) (width 0.12))
  (fp_line (start -3.5 6.6) (end -3.5 8) (layer F.CrtYd) (width 0.12))
  (fp_line (start -3.5 8) (end -1.9 8) (layer F.CrtYd) (width 0.12))
  (fp_line (start -1.9 8) (end -1.9 10.6) (layer F.CrtYd) (width 0.12))
  (fp_line (start -1.9 10.6) (end 1.9 10.6) (layer F.CrtYd) (width 0.12))
  (fp_line (start 1.9 10.6) (end 1.9 8) (layer F.CrtYd) (width 0.12))
  (fp_line (start 1.9 8) (end 3.5 8) (layer F.CrtYd) (width 0.12))
  (fp_line (start 3.5 8) (end 3.5 -1.1) (layer F.CrtYd) (width 0.12))
  (fp_line (start 3.5 -1.1) (end 5.6 -1.1) (layer F.CrtYd) (width 0.12))
  (pad "" np_thru_hole circle (at 0 -3.5) (size 1.6 1.6) (drill 1.6) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 0 3.5) (size 1.6 1.6) (drill 1.6) (layers *.Cu *.Mask))
  (pad TN smd rect (at 0 8.8) (size 2.7 2.6) (layers F.Cu F.Paste F.Mask))
  (pad T smd rect (at -4.05 4.7) (size 2.1 2.7) (layers F.Cu F.Paste F.Mask))
  (pad S smd rect (at -4.05 -4.6) (size 2.1 2.2) (layers F.Cu F.Paste F.Mask))
  (pad R smd rect (at 4.05 -2.7) (size 2.1 2.2) (layers F.Cu F.Paste F.Mask))
  (pad RN smd rect (at 4.05 -5.4) (size 2.1 2.2) (layers F.Cu F.Paste F.Mask))
)
