(module Buzzer_TDK_PS1440P02BT_D14mm_H8mm (layer F.Cu) (tedit 5E8CBE59)
  (descr "Buzzer, D14mm height 8mm, https://product.tdk.com/info/en/catalog/datasheets/piezoelectronic_buzzer_ps_en.pdf")
  (tags buzzer)
  (fp_text reference REF** (at 2.5 -7.95) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Buzzer_TDK_PS1440P02BT_D14mm_H8mm (at 2.45 8.15) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_arc (start 2.5 0) (end -4.6 -1.5) (angle -25.11993457) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.3 -1) (end -1.3 1) (layer F.Fab) (width 0.1))
  (fp_circle (center 2.5 0) (end 9.5 0) (layer F.SilkS) (width 0.12))
  (fp_circle (center 2.5 0) (end 3.5 0) (layer F.Fab) (width 0.1))
  (fp_circle (center 2.5 0) (end 9.35 0) (layer F.Fab) (width 0.1))
  (fp_circle (center 2.5 0) (end 9.6 0) (layer F.CrtYd) (width 0.05))
  (fp_text user %R (at 2.5 -2.43) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad 2 thru_hole circle (at 5 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/Buzzer_Beeper.3dshapes/Buzzer_TDK_PS1240P02BT_D12.2mm_H6.5mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
