(footprint "PanelCutout_LED_0603_1608Metric_SideView_Inolux" (version 20201116) (generator pcbnew) (layer "F.Cu")
  (tedit 5FC9F963)
  (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 48de3760-f742-4637-90ec-3ad872c57f18)
  )
  (fp_text value "PanelCutout_LED_0603_1608Metric_SideView_Inolux" (at 0 1 unlocked) (layer "F.Fab") hide
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 4ee8696e-d3bd-445e-a302-0681ff22d30f)
  )
  (fp_text user "${REFERENCE}" (at 0 1.4 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 6ddbea47-b25e-42ea-a8df-f4e8f38a9417)
  )
  (fp_line (start 0.85 0.3) (end 0.75 0.3) (layer "F.SilkS") (width 0.12) (tstamp 14de2fd0-733a-417f-acf3-519ae8835746))
  (fp_line (start 0.85 -0.3) (end 0.85 0.3) (layer "F.SilkS") (width 0.12) (tstamp 2d46a45e-80a3-4194-828d-c222ab9013ca))
  (fp_line (start -0.85 -0.3) (end -0.75 -0.3) (layer "F.SilkS") (width 0.12) (tstamp 312b793c-c493-45c0-8458-333aef6069a0))
  (fp_line (start 0.85 -0.3) (end 0.75 -0.3) (layer "F.SilkS") (width 0.12) (tstamp 6dd4f922-cec7-4595-9e22-05a3911132bf))
  (fp_line (start -0.85 0.3) (end -0.85 -0.3) (layer "F.SilkS") (width 0.12) (tstamp 9734e07c-f82d-48a0-92c5-08b74ba7aa6c))
  (fp_line (start -0.85 0.3) (end -0.75 0.3) (layer "F.SilkS") (width 0.12) (tstamp c17277fa-a33c-40a1-be8a-4503a8267828))
  (fp_rect (start -0.9 -0.9) (end 0.9 0.9) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp 2b58bbf9-ccff-4c4c-b749-bc54b17f93db))
  (fp_rect (start -0.85 -0.3) (end 0.85 0.3) (layer "F.Fab") (width 0.1) (fill none) (tstamp fa8db335-bafd-4fa0-882c-8701207ed9c6))
  (pad "" np_thru_hole circle (at 0 0) (size 1.3 1.3) (drill 1.3) (layers *.Mask) (tstamp a7dec3f3-863c-47a1-b4f9-001f58955994))
  (model "${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
    (offset (xyz 0 0 1))
    (scale (xyz 1 1 1))
    (rotate (xyz -180 0 0))
  )
)
