(footprint "TexasInstruments_DAP32" (version 20201116) (generator pcbnew) (layer "F.Cu")
  (tedit 5FC96BEA)
  (attr smd)
  (fp_text reference "REF**" (at 0 6.3 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp c2b9f73f-d8c4-4ec1-ba9e-412ee9fbd679)
  )
  (fp_text value "TexasInstruments_DAP32" (at 5.4 0 90 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 5d480cd6-8749-418f-adc0-1c6a84dbd7b2)
  )
  (fp_text user "${REFERENCE}" (at 0.1 0 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp beef71e6-8b28-4be8-96e4-ca34b31cd9d5)
  )
  (fp_line (start 3.05 -5.5) (end -4.5 -5.5) (layer "F.SilkS") (width 0.12) (tstamp 37d3c421-77a7-408f-b374-4ee4f701a179))
  (fp_line (start 3.05 5.5) (end 3.05 -5.5) (layer "F.SilkS") (width 0.12) (tstamp 3e1fa182-71fa-4693-afba-3a81c20380d1))
  (fp_line (start -3.05 -5.5) (end -3.05 5.5) (layer "F.SilkS") (width 0.12) (tstamp c39fa827-df17-4f40-8901-4e94f91fb7ed))
  (fp_line (start -3.05 5.5) (end 3.05 5.5) (layer "F.SilkS") (width 0.12) (tstamp c53472aa-60bc-435e-908f-69ad22c4a06b))
  (pad "1" smd rect (at -3.7 -4.875 270) (size 0.3 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 3c1a0b3a-c2de-4b59-8ab8-4ec291eeea24))
  (pad "2" smd rect (at -3.7 -4.225 270) (size 0.3 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp c5a7f7b9-5764-49cb-9e5c-166af95f27cb))
  (pad "3" smd rect (at -3.7 -3.575 270) (size 0.3 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp eb61e7e3-90a2-43bb-a988-98ad36e9d472))
  (pad "4" smd rect (at -3.7 -2.925 270) (size 0.3 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 60983501-3983-4605-ba13-d5c4d7c2246c))
  (pad "5" smd rect (at -3.7 -2.275 270) (size 0.3 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 4245c2df-fd04-474f-aa7f-8736bf84b571))
  (pad "6" smd rect (at -3.7 -1.625 270) (size 0.3 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 5b18f4e0-61d7-45d1-8cb3-ef4d3d9d0a61))
  (pad "7" smd rect (at -3.7 -0.975 270) (size 0.3 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 13549d47-e73a-42aa-ad59-32ef51e7ad25))
  (pad "8" smd rect (at -3.7 -0.325 270) (size 0.3 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 0fbc85d3-28f1-40d7-8a0c-4cb40c6d8085))
  (pad "9" smd rect (at -3.7 0.325 270) (size 0.3 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 4c38dab8-6799-470f-8ff8-af3ec94b284f))
  (pad "10" smd rect (at -3.7 0.975 270) (size 0.3 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 66743517-ca6e-4115-b391-58bc24e252b8))
  (pad "11" smd rect (at -3.7 1.625 270) (size 0.3 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp b201f28e-2198-4f32-9afa-b8144d5c1f8e))
  (pad "12" smd rect (at -3.7 2.275 270) (size 0.3 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp bc9e02c0-217c-4d6d-9350-fff85713dab3))
  (pad "13" smd rect (at -3.7 2.925 270) (size 0.3 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 4cb9617f-6515-456f-aa03-e3ccbaf556ae))
  (pad "14" smd rect (at -3.7 3.575 270) (size 0.3 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 4ccd9d49-0d9c-4707-8937-7dc170eec234))
  (pad "15" smd rect (at -3.7 4.225 270) (size 0.3 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 36a970df-00de-4dba-a217-0272ab52731f))
  (pad "16" smd rect (at -3.7 4.875 270) (size 0.3 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp cdede079-9948-46df-b063-7e07d78063ab))
  (pad "17" smd rect (at 3.7 4.875 270) (size 0.3 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 35067842-8ab0-4bfb-bc78-2cf5b8243038))
  (pad "18" smd rect (at 3.7 4.225 270) (size 0.3 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 3c130787-add4-46f9-83d1-a2f6a8f5c1be))
  (pad "19" smd rect (at 3.7 3.575 270) (size 0.3 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp f11da863-65f7-4680-8c90-f0e4b8250050))
  (pad "20" smd rect (at 3.7 2.925 270) (size 0.3 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp fcfc1998-f589-4efb-b7ac-b2ebb9415a47))
  (pad "21" smd rect (at 3.7 2.275 270) (size 0.3 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp c07ef785-7ac1-4857-80df-52e9602cd312))
  (pad "22" smd rect (at 3.7 1.625 270) (size 0.3 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 1804bc51-87ef-49af-9ebd-a3e66455ef3e))
  (pad "23" smd rect (at 3.7 0.975 270) (size 0.3 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 23ebe93f-c0d0-4d88-bdd7-e508f1633d09))
  (pad "24" smd rect (at 3.7 0.325 270) (size 0.3 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp c2aa26d7-c259-44c8-bc04-f82d7b35a5ee))
  (pad "25" smd rect (at 3.7 -0.325 270) (size 0.3 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 36a89ee6-bf90-4766-9fc2-8c78efa29b8a))
  (pad "26" smd rect (at 3.7 -0.975 270) (size 0.3 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 430a4230-72ed-4c05-a9f8-d0b5e5fae190))
  (pad "27" smd rect (at 3.7 -1.625 270) (size 0.3 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 0aaf1bf6-07c1-42f2-bad7-1e2138c515f7))
  (pad "28" smd rect (at 3.7 -2.275 270) (size 0.3 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp ad56d18e-386c-4c5a-b6d3-ed63e28620f1))
  (pad "29" smd rect (at 3.7 -2.925 270) (size 0.3 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 06eeee7d-8f26-42d0-86bf-584a9ac3d6b1))
  (pad "30" smd rect (at 3.7 -3.575 270) (size 0.3 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp deae3f3b-a6c7-4931-ab53-11b9a6661cfb))
  (pad "31" smd rect (at 3.7 -4.225 270) (size 0.3 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp f629d9bb-4dfe-4bef-9276-f99752307b70))
  (pad "32" smd rect (at 3.7 -4.875 270) (size 0.3 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 4bed3e3a-42b2-4fb2-b6bf-8d0408793fa1))
  (pad "33" thru_hole circle (at -2 -3 270) (size 0.5 0.5) (drill 0.33) (layers *.Cu *.Mask "F.SilkS")
    (zone_connect 2) (tstamp 0451a70a-c39b-478a-b018-f02ff431cdb2))
  (pad "33" thru_hole circle (at 0 4 270) (size 0.5 0.5) (drill 0.33) (layers *.Cu *.Mask "F.SilkS")
    (zone_connect 2) (tstamp 0e5bd1ce-fc45-42b2-af52-b3d9ae7dd578))
  (pad "33" thru_hole circle (at -2 4 270) (size 0.5 0.5) (drill 0.33) (layers *.Cu *.Mask "F.SilkS")
    (zone_connect 2) (tstamp 0f86680e-528d-47cb-98da-7b5ed4ddfade))
  (pad "33" thru_hole circle (at 1 -4) (size 0.5 0.5) (drill 0.33) (layers *.Cu *.Mask "F.SilkS")
    (zone_connect 2) (tstamp 14255d90-e0bc-48a9-ab95-88221aad85e5))
  (pad "33" thru_hole circle (at 1.5 1.5) (size 0.5 0.5) (drill 0.33) (layers *.Cu *.Mask "F.SilkS")
    (zone_connect 2) (tstamp 151f2b01-a7b7-403b-b65b-775b7e78763c))
  (pad "33" thru_hole circle (at -1 3 270) (size 0.5 0.5) (drill 0.33) (layers *.Cu *.Mask "F.SilkS")
    (zone_connect 2) (tstamp 18f38687-07f5-4243-b795-8cf855976ed9))
  (pad "33" thru_hole circle (at 0 5 270) (size 0.5 0.5) (drill 0.33) (layers *.Cu *.Mask "F.SilkS")
    (zone_connect 2) (tstamp 2ca929cd-ee48-4512-979a-02a4cf4f85d2))
  (pad "33" thru_hole circle (at 1.5 0.5) (size 0.5 0.5) (drill 0.33) (layers *.Cu *.Mask "F.SilkS")
    (zone_connect 2) (tstamp 2d5c0d40-2592-407d-ad6b-14997b7a9b14))
  (pad "33" thru_hole circle (at 0.5 -0.5 270) (size 0.5 0.5) (drill 0.33) (layers *.Cu *.Mask "F.SilkS")
    (zone_connect 2) (tstamp 308f097e-53c2-4f89-a0e6-14bd8e6fe219))
  (pad "33" thru_hole circle (at 2 -5) (size 0.5 0.5) (drill 0.33) (layers *.Cu *.Mask "F.SilkS")
    (zone_connect 2) (tstamp 33bc2f73-9aa7-484d-b36a-1ee5a300ca47))
  (pad "33" thru_hole circle (at -2 -5 270) (size 0.5 0.5) (drill 0.33) (layers *.Cu *.Mask "F.SilkS")
    (zone_connect 2) (tstamp 361dabce-0a66-4e23-97ec-dba53cd3ad38))
  (pad "33" thru_hole circle (at -0.5 1.5 270) (size 0.5 0.5) (drill 0.33) (layers *.Cu *.Mask "F.SilkS")
    (zone_connect 2) (tstamp 3a075697-8b91-48a6-800e-a13ff3e869a7))
  (pad "33" thru_hole circle (at 0.5 1.5 270) (size 0.5 0.5) (drill 0.33) (layers *.Cu *.Mask "F.SilkS")
    (zone_connect 2) (tstamp 40526c47-f3c7-4153-b8c5-45d7497531bf))
  (pad "33" thru_hole circle (at -1 5 270) (size 0.5 0.5) (drill 0.33) (layers *.Cu *.Mask "F.SilkS")
    (zone_connect 2) (tstamp 4756b853-c64e-42fd-980d-1255eb98acaa))
  (pad "33" thru_hole circle (at -1 -3 270) (size 0.5 0.5) (drill 0.33) (layers *.Cu *.Mask "F.SilkS")
    (zone_connect 2) (tstamp 4f44c105-114a-4574-8560-1f0ebb6a21c5))
  (pad "33" thru_hole circle (at -1 4 270) (size 0.5 0.5) (drill 0.33) (layers *.Cu *.Mask "F.SilkS")
    (zone_connect 2) (tstamp 4f94cd78-9bbf-476b-9d55-37a82499bc22))
  (pad "33" thru_hole circle (at 1 4) (size 0.5 0.5) (drill 0.33) (layers *.Cu *.Mask "F.SilkS")
    (zone_connect 2) (tstamp 53f4c3a8-f27b-4428-8960-1bb37c723814))
  (pad "33" thru_hole circle (at 2 3) (size 0.5 0.5) (drill 0.33) (layers *.Cu *.Mask "F.SilkS")
    (zone_connect 2) (tstamp 560066ce-d2ec-4953-a500-f5163e0be30d))
  (pad "33" thru_hole circle (at -2 -4 270) (size 0.5 0.5) (drill 0.33) (layers *.Cu *.Mask "F.SilkS")
    (zone_connect 2) (tstamp 56b7a4c8-aa42-4650-a15b-a9743bc387a6))
  (pad "33" thru_hole circle (at -0.5 -1.5 270) (size 0.5 0.5) (drill 0.33) (layers *.Cu *.Mask "F.SilkS")
    (zone_connect 2) (tstamp 663e693f-123c-4f74-a06c-d2e7363e6154))
  (pad "33" thru_hole circle (at -0.5 -0.5 270) (size 0.5 0.5) (drill 0.33) (layers *.Cu *.Mask "F.SilkS")
    (zone_connect 2) (tstamp 67d793f9-fa3e-4e32-93be-c6df535de7d6))
  (pad "33" thru_hole circle (at -0.5 0.5 270) (size 0.5 0.5) (drill 0.33) (layers *.Cu *.Mask "F.SilkS")
    (zone_connect 2) (tstamp 6ee695f7-3d6c-44ce-9034-97e2fdf3cbe7))
  (pad "33" thru_hole circle (at -2 3 270) (size 0.5 0.5) (drill 0.33) (layers *.Cu *.Mask "F.SilkS")
    (zone_connect 2) (tstamp 70d16193-6596-44ee-872c-df68d5c54d9f))
  (pad "33" thru_hole circle (at -1 -4 270) (size 0.5 0.5) (drill 0.33) (layers *.Cu *.Mask "F.SilkS")
    (zone_connect 2) (tstamp 7388a677-4e51-47b8-b50c-bf19a8be38f8))
  (pad "33" thru_hole circle (at -2 5 270) (size 0.5 0.5) (drill 0.33) (layers *.Cu *.Mask "F.SilkS")
    (zone_connect 2) (tstamp 7d669c1d-a259-4e3a-88be-ab5144fe44cd))
  (pad "33" thru_hole circle (at 0 -5 270) (size 0.5 0.5) (drill 0.33) (layers *.Cu *.Mask "F.SilkS")
    (zone_connect 2) (tstamp 7dff3173-b414-4b49-a3fb-6203c57103a6))
  (pad "33" smd rect (at 0 0 270) (size 4.36 4.11) (layers "F.Cu" "F.Paste" "F.Mask")
    (zone_connect 2) (tstamp 80e6de6e-73c1-465d-a0b8-1b62e3a62700))
  (pad "33" thru_hole circle (at 2 5) (size 0.5 0.5) (drill 0.33) (layers *.Cu *.Mask "F.SilkS")
    (zone_connect 2) (tstamp 80f3a66e-dc87-4fc2-a85c-a752c0acc88f))
  (pad "33" thru_hole circle (at -1.5 0.5 270) (size 0.5 0.5) (drill 0.33) (layers *.Cu *.Mask "F.SilkS")
    (zone_connect 2) (tstamp 98092bad-17c7-4a75-8ca7-4b6bd4485f04))
  (pad "33" thru_hole circle (at 1.5 -1.5) (size 0.5 0.5) (drill 0.33) (layers *.Cu *.Mask "F.SilkS")
    (zone_connect 2) (tstamp 9db85ce1-6c60-496d-9bea-d21a50f6cc22))
  (pad "33" thru_hole circle (at 1.5 -0.5) (size 0.5 0.5) (drill 0.33) (layers *.Cu *.Mask "F.SilkS")
    (zone_connect 2) (tstamp aa6d0e2d-d4e4-41e6-8182-35b0d99db1ff))
  (pad "33" thru_hole circle (at 2 -4) (size 0.5 0.5) (drill 0.33) (layers *.Cu *.Mask "F.SilkS")
    (zone_connect 2) (tstamp aab719a5-e86e-4044-93e0-b53bd0d0b6a2))
  (pad "33" thru_hole circle (at 1 -3) (size 0.5 0.5) (drill 0.33) (layers *.Cu *.Mask "F.SilkS")
    (zone_connect 2) (tstamp adbb5137-39ba-495f-9a50-3cc1fc625e25))
  (pad "33" thru_hole circle (at 1 3) (size 0.5 0.5) (drill 0.33) (layers *.Cu *.Mask "F.SilkS")
    (zone_connect 2) (tstamp ae396207-8067-4711-8db5-d5d8a58842fe))
  (pad "33" thru_hole circle (at -1.5 1.5 270) (size 0.5 0.5) (drill 0.33) (layers *.Cu *.Mask "F.SilkS")
    (zone_connect 2) (tstamp aeb0b1be-a2e4-4a34-b9bd-907c346e42b6))
  (pad "33" thru_hole circle (at 2 -3) (size 0.5 0.5) (drill 0.33) (layers *.Cu *.Mask "F.SilkS")
    (zone_connect 2) (tstamp b4728e94-f877-476f-9a1e-524d175c5684))
  (pad "33" thru_hole circle (at -1 -5 270) (size 0.5 0.5) (drill 0.33) (layers *.Cu *.Mask "F.SilkS")
    (zone_connect 2) (tstamp bba49445-ea53-4bde-b46f-18983182bba5))
  (pad "33" thru_hole circle (at 0.5 0.5 270) (size 0.5 0.5) (drill 0.33) (layers *.Cu *.Mask "F.SilkS")
    (zone_connect 2) (tstamp c07fc542-4832-46a8-b88d-f1e92b8ff8e9))
  (pad "33" thru_hole circle (at 0 -4 270) (size 0.5 0.5) (drill 0.33) (layers *.Cu *.Mask "F.SilkS")
    (zone_connect 2) (tstamp c1f84248-5f76-46d3-8c75-b7eea715b852))
  (pad "33" thru_hole circle (at 2 4) (size 0.5 0.5) (drill 0.33) (layers *.Cu *.Mask "F.SilkS")
    (zone_connect 2) (tstamp d15d1e57-7391-4f99-a597-cf1948df764c))
  (pad "33" thru_hole circle (at -1.5 -1.5 270) (size 0.5 0.5) (drill 0.33) (layers *.Cu *.Mask "F.SilkS")
    (zone_connect 2) (tstamp dfd26b1a-cceb-499b-8562-db68ea197c50))
  (pad "33" thru_hole circle (at 1 -5) (size 0.5 0.5) (drill 0.33) (layers *.Cu *.Mask "F.SilkS")
    (zone_connect 2) (tstamp e8aca527-3b42-46b8-b72a-c7fe99a7512a))
  (pad "33" thru_hole circle (at 0.5 -1.5 270) (size 0.5 0.5) (drill 0.33) (layers *.Cu *.Mask "F.SilkS")
    (zone_connect 2) (tstamp e95bcc22-7bc7-404c-80ca-3e837092f4ac))
  (pad "33" thru_hole circle (at 0 3 270) (size 0.5 0.5) (drill 0.33) (layers *.Cu *.Mask "F.SilkS")
    (zone_connect 2) (tstamp eb526746-463e-4da4-8bb9-4741c6cde094))
  (pad "33" thru_hole circle (at 0 -3 270) (size 0.5 0.5) (drill 0.33) (layers *.Cu *.Mask "F.SilkS")
    (zone_connect 2) (tstamp ecdd9891-29b4-48b2-8d41-ae87c06cd77e))
  (pad "33" thru_hole circle (at 1 5) (size 0.5 0.5) (drill 0.33) (layers *.Cu *.Mask "F.SilkS")
    (zone_connect 2) (tstamp f4eabe3d-3429-49ea-ace1-5363c828e35e))
  (pad "33" thru_hole circle (at -1.5 -0.5 270) (size 0.5 0.5) (drill 0.33) (layers *.Cu *.Mask "F.SilkS")
    (zone_connect 2) (tstamp fd7956d7-6b8f-4fd3-b762-04e4be3adb22))
  (model "/home/mathias/Projects/microcontroller/HackAmp/3dmodels/DAP0032B.stp"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
