(footprint "PanelCutout_SW_PUSH_6mm_Angled" (version 20201116) (generator pcbnew) (layer "F.Cu")
  (tedit 5FC2117E)
  (fp_text reference "REF**" (at 0 -3.75 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp eeedfed6-8dd7-4578-93b0-50c7b582c845)
  )
  (fp_text value "PanelCutout_SW_PUSH_6mm_Angled" (at 0 -5.15 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 622d064f-3060-4c76-ba1b-63a0031fd83f)
  )
  (fp_text user "${REFERENCE}" (at 0 -3.75 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp d4b3d7c1-ccf8-4457-9d12-401c65826eaa)
  )
  (fp_rect (start -3 -3) (end 3 3) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 77135839-6e38-4978-b266-5400cfa23c4d))
  (fp_rect (start -4.05 -3.5) (end 4.05 8) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp d099f986-e775-4d38-90b5-3beb54738400))
  (fp_line (start -3.55 4) (end -3.55 7.5) (layer "F.Fab") (width 0.1) (tstamp 3538e8ca-7b33-4b1d-9c38-1ee8d9939988))
  (fp_line (start 3.55 4) (end 3.55 7.5) (layer "F.Fab") (width 0.1) (tstamp f1ead84e-dec7-4655-99c8-04bf9374b669))
  (fp_rect (start -3.55 -3) (end 3.55 4) (layer "F.Fab") (width 0.1) (fill none) (tstamp 6fd3c5cc-2d8a-4483-97ec-3efe94fc3795))
  (pad "" np_thru_hole circle (at 0 0) (size 3.7 3.7) (drill 3.7) (layers *.Mask) (tstamp 09411be9-a27f-47d6-a068-e1d01f9f3c79))
  (model "/home/mathias/Projects/microcontroller/HackAmp/3dmodels/c-2-1825027-0-g-3d.stp"
    (offset (xyz 0 0 0.3))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 180 0))
  )
)
