(footprint "PanelCutout_Vishay_Mold" (version 20201116) (generator pcbnew) (layer "F.Cu")
  (tedit 5FC20C5E)
  (fp_text reference "REF**" (at 0 -3.45 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 8126c794-859c-497e-9857-00758117811c)
  )
  (fp_text value "PanelCutout_Vishay_Mold" (at 0 -4.85 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 72f7d9da-a68f-448e-838d-3f4673093635)
  )
  (fp_text user "${REFERENCE}" (at 0 -3.45 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp b59215e2-040a-4abf-a18d-211bcfd1acb0)
  )
  (fp_rect (start -3 -2.7) (end 3 4.25) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 8f84c1aa-c88b-4e4e-b2db-20dabfce0317))
  (fp_rect (start -3.5 -3.2) (end 3.5 7.75) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp d659ebc0-ee86-4426-baa3-96c2aed1861d))
  (fp_line (start -3 5.55) (end 3 5.55) (layer "F.Fab") (width 0.1) (tstamp 1e44274b-70a2-4612-852b-9cd0a213f482))
  (fp_rect (start -2.2 4.25) (end -2.9 7.25) (layer "F.Fab") (width 0.1) (fill none) (tstamp 18c9ff11-50a4-45d6-be43-29cb4bb3f333))
  (fp_rect (start -3 -2.7) (end 3 4.25) (layer "F.Fab") (width 0.1) (fill none) (tstamp 8efdc589-262b-4022-ac1b-1ee38a1e54d3))
  (fp_rect (start 0.35 4.25) (end -0.35 7.25) (layer "F.Fab") (width 0.1) (fill none) (tstamp c150e0cc-62e2-45df-ad44-889c767940c5))
  (fp_rect (start 2.2 4.25) (end 2.9 7.25) (layer "F.Fab") (width 0.1) (fill none) (tstamp eeaa976d-78e4-4119-bcea-b3447032dd83))
  (pad "" np_thru_hole circle (at 0 0) (size 5 5) (drill 5) (layers *.Mask) (tstamp fd3782d3-0735-496a-9c11-4bc1b04abe01))
  (model "${KISYS3DMOD}/OptoDevice.3dshapes/Vishay_MOLD-3Pin.wrl"
    (offset (xyz 2.54 -7.62 3.05))
    (scale (xyz 1 1 1))
    (rotate (xyz 90 180 0))
  )
)
