(footprint "PanelCutout_RotaryEncoder_TT_EN12-V_Knob16mm" (version 20201116) (generator pcbnew) (layer "F.Cu")
  (tedit 5FCABB13)
  (fp_text reference "REF**" (at 0 -4.5 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp cbb1abd5-6ab5-45c3-b9cd-8618ca18e096)
  )
  (fp_text value "PanelCutout_RotaryEncoder_TT_EN12-V_Knob16mm" (at 0 6 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 2c9b2340-1094-44e2-9110-f3b8998355c7)
  )
  (fp_text user "${REFERENCE}" (at 0 4.5 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 31a4de90-b549-44ea-9558-c2dc01e33bad)
  )
  (fp_line (start -6.2 10) (end 6.2 10) (layer "F.SilkS") (width 0.12) (tstamp 193420aa-932e-46bc-b274-58ce1bcf56a0))
  (fp_rect (start -6.2 -6.6) (end 6.2 6.6) (layer "F.SilkS") (width 0.12) (fill none) (tstamp d1937bd4-45d8-4646-937d-e2b589d37fd0))
  (fp_circle (center 0 0) (end 8.5 0) (layer "B.CrtYd") (width 0.05) (fill none) (tstamp 233ff8da-5455-4fb3-9c9e-9ee1d1ca6c34))
  (fp_rect (start -6.7 10.5) (end 6.7 -7.1) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp a353b4f6-067a-473c-bf7a-7f6824a1e516))
  (fp_line (start -6.2 6.6) (end -6.2 13.5) (layer "F.Fab") (width 0.1) (tstamp 40be51f0-f05f-4e3e-a46a-a99b4246edfa))
  (fp_line (start 6.2 6.6) (end 6.2 13.5) (layer "F.Fab") (width 0.1) (tstamp e56ecc5e-f1c8-4891-9436-64118d4adff1))
  (fp_rect (start -6.2 -6.6) (end 6.2 6.6) (layer "F.Fab") (width 0.1) (fill none) (tstamp 519d34a4-afd3-4a65-ad3e-62f2d136ad19))
  (fp_circle (center 0 0) (end 8 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp 6985e2b7-4dd5-47fb-a3b7-bcb954628bcf))
  (pad "" np_thru_hole circle (at 0 0) (size 7.2 7.2) (drill 7.2) (layers *.Mask) (tstamp 9aac4df8-de23-4256-9ffd-895efc8f2f15))
  (model "/home/mathias/Projects/microcontroller/HackAmp/3dmodels/EN12-VS11AF18.stp"
    (offset (xyz -3 3 4.8))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 90))
  )
)
